

Business To Manufacturing   
Markup Language

Production Schedule

Version 0700

August 5, 2016

B2MML-ProductionSchedule

IMPORTANT: While the information, data, and standards provided in this publication were developed and are presented in good faith in accordance with a reasonable process that was subject to intellectual property and antitrust policies to benefit the industry as a whole, the publication is provided “as is” for information and guidance only, and there is no representation or warranty of any type or kind, including but not limited to warranties of merchantability or fitness for a particular purpose, and no warranty that use of the information, data, or standards will not infringe patent, copyright, trademark, trade secret, or other intellectual property rights of any party.

Copyright © 2016 MESA International

All Rights Reserved. http://www.mesa.org

This MESA Work (including specifications, documents, software, and related items) referred to as the Business To Manufacturing Markup Language (B2MML) is provided by the copyright holders under the following license.

Permission to use, copy, modify, or redistribute this Work and its documentation, with or without modification, for any purpose and without fee or royalty is hereby granted provided MESA International is acknowledged as the originator of this Work using the following statement:

"The Business To Manufacturing Markup Language (B2MML) is used courtesy of MESA International."

In no event shall MESA International, its members, or any third party be liable for any costs, expenses, losses, damages or injuries incurred by use of the Work or as a result of this agreement.

Material from ANSI/ISA-88 and ANSI/ISA-95 series of standards used with permission of ISA - The Instrumentation, Systems, and Automation Society, www.isa.org

Table of Contents

­

Change history 3

Schema Scope 4

Key Information Assumptions 4

ProductionSchedule 5

ProductionRequest 5

SegmentRequirement 5

SegmentResponse 5

PersonnelRequirement 6

EquipmentRequirement 6

PhysicalAssetRequirement 6

MaterialRequirement 6

MaterialProducedRequirement 6

MaterialsConsumedRequirement 6

ConsumableExpectedRequirement 7

Resource Identification 7

Element Definitions 8

Transaction Elements 17

Diagram Convention 18

# Change history

|  |  |  |  |
| --- | --- | --- | --- |
| **Change** | **Date** | **Person** | **Description** |
| V01 | 7 April 2002 | Dennis Brandl  Dave Emerson | Initial release |
| V02 | 23 Sept 2003 | Dennis Brandl  Dave Emerson | * Fixed the missing unbounded on the description in *MaterialConsumedRequirementType* * Added *RequiredByRequestedSegmentResponse* to * *SegmentRequirementType* and sub elements * Changed ##any to "Any" element of type "AnyType" * Removed include of Common schema since it is included when *ProductionPerformance* schema is included |
| V03 | 26 Aug 2005 | Dennis Brandl  Dave Emerson | * Added substitution groups. One group added just before each Any element. |
| V0301 | 29 Dec 2005 | Dennis Brandl | * Changed “Value” elements to 0..unbounded |
| V04 | 04 June 2007 | Dennis Brandl | * Added transaction elements and MaterialRequirement as replacement for produced, consumed, and consumable materials. |
| V0401 | Oct 2008 | Dennis Brandl | * Changed maxOccurs for resource elements in Segment Requirements |
| V0500 | Mar 2011 | Dennis Brandl | * Updated for ISA 95.02-2010 changes * Added physical asset elements * Added material assembly elements * Removed AnyType |
| V0600 | Aug 2012 | D. Brandl | Updated MESA Copyright |
| V0700 | Aug 2016 | D. Brandl | Updated version number only |

# Schema Scope

This document defines the information about production schedules sent from business systems to manufacturing operations systems. This information is based on the data models and attributes defined in the ANSI/ISA 95.00.02 Enterprise/Control System Integration standard. Contact ISA (The Instrumentation, System, and Automation Society) for copies of the standard. Additional information on the standard is available at [www.isa.org](http://www.isa.org).

## Key Information Assumptions

The data represented in these schemas is derived from the UML model below. This model is an extension of the model defined in the ANSI/ISA 95.00.02 standard, and is based on the planned update of the ANSI/ISA standard. The information model in the figure below is hierarchical, and the assumption is that any production request information will always be within a contained production schedule object.

The Material Requirement object is a replacement for the Material Produced Requirement, Material Consumed Requirement, and Consumable Expected objects.



Model of Exchanged Production Schedule Information

This schema uses a common schema for definition of elements that are used in multiple schemas, such as ID, Description, and Value. This schema also includes the Production Performance schema definition for the requested segment response structure. See the document defining the Common schema for definition of the common elements. See the document defining the Production Performance schema for the definition of the requested segment response.

## ProductionSchedule

A production schedule is made up of a set of 1 or more production requests. The production schedule also contains the information that defines the context of the schedule, such as start time, end time, location, and published date. The main structuring element of the schema definition is ProductionSchedule.

## ProductionRequest

A production request defines a request for production for a single product identified by a production rule. A production request contains the information required by manufacturing to fulfill scheduled production. This may be a subset of the business production order information, or it may contain additional information not normally used by the business system.

A production request identifies the associated production rule. A production request must contain at least one segment requirement, even it spans all production of the product. If not uniquely defined by the production rule, then a segment requirement will contain at least one material produced requirement with the identification, quantity, and units of measure of the material to be produced.

## SegmentRequirement

A production request is made up of one or more segment requirements. Each segment requirement may correspond to, or reference, an identified process or product segment. The segment requirement references the segment capability to which the associated personnel, equipment, materials, and production parameters correspond.

A SegmentRequirement reflects the ISA-95 standard where it says that a segment requirement corresponds to either a product segment or a process segment. It many cases it may not matter. A segment request should define resources and parameters already defined in process segments or product segments. However, in general in order to match the spirit of the ANSI/ISA-95 standard, this should always be a product segment ID in the SegmentRequirement, and the product segment should refer to a process segment through the ProductDefinition.

The production parameter in a SegmentRequirement can be a Process Segment parameter, or a Product Segment parameter. This means the production parameter could have been defined in the process segment, because it is product independent (like the color in a "PAINT" segment), or defined in a product segment when it is product dependent (such as a component’s color to be applied to only specific products). So, the SegmentRequirement could point to the product segment, but there could possible be duplicated parameters for the product segment and the process segment, and this allows them to be differentiated.

## SegmentResponse

A production request may include a SegmentResponse element that defines the data to be returned after the execution of the segment.

NOTE: The SegmentResponse element (SegmentResponseType) is defined in the file:

**B2MML-V0601-ProductionPerformanceTypes.xsd**

## PersonnelRequirement

A personnel requirement and the associated personnel requirement property elements define to the number, type, duration, and scheduling of specific certifications and job classifications needed to support the current production request.

## EquipmentRequirement

The production request may include one or more requirements for, or constraints upon, the equipment that the facility shall use in the production process for the scheduled item. Requirements can be as generic as materials of construction, or it can as specific as a particular piece of equipment. Each of these requirements is defined in an EquipmentRequirement element and property.

## PhysicalAssetRequirement

The production request may include one or more requirements for, or constraints upon, the physical assets that the facility shall use in the production process for the scheduled item. Requirements can be as generic as materials of construction, or it can as specific as a particular physical asset. Each of these requirements is defined in a PhysicalAssetRequirement element and property.

## MaterialRequirement

A MaterialRequirement defines a requirement for a material to be produced, a material that will be consumed, or the expected amount of a consumable material. A material requirement may include the total quantity of the material to be produced or consumed and unit of measure, such as 5000 Lbs, and an acceptable range for the quantity of material. Material may be defined by Material Class ID, Material Definition ID, Material Lot ID, and/or Material Sublot ID. A MaterialRequirement element includes an element that specifies if the material is to be consumed, produced, or is a consumable material

## MaterialProducedRequirement

A material produced requirement is an identification of a material to be produced from the production request. A material produced requirement may include the total quantity of the material to be produced and unit of measure, such as 5000 Lbs, and an acceptable range for the quantity of material. Material may be defined by Material Class ID, Material Definition ID, Material Lot ID, and/or Material Sublot ID.

Specific elements associated with each material produced requirement may be included in one or more material produced requirement properties.

Note: This element is included for backward compatibility. The MaterialRequirement should be used to specify material requirements.

## MaterialsConsumedRequirement

A material consumed requirement is an identification of a material to be used in the production request. A material consumed requirement may include the total quantity of the material to be used and unit of measure, such as 5000 Lbs, and an acceptable range for the quantity of material. Material may be defined by Material Class ID, Material Definition ID, Material Lot ID, and/or Material Sublot ID.

Specific elements associated with each material consumed requirement may be included in one or more material consumed requirement properties.

Note: This element is included for backward compatibility. The MaterialRequirement should be used to specify material requirements.

## ConsumableExpectedRequirement

Consumable expected include resources that are not normally included in bills of materials or are not individually accounted for in specific production requests. Depending on the industry these may include water, catalysts, common chemicals, and utilities, such as electricity and steam. These items will often result in direct charges that will usually be considered in costing the product segment. Consumables are often materials that do have an inventory balance.

Consumables do not have lot identifications. Consumables with lot identifications are typically treated as material consumed requirements.

Note: This element is included for backward compatibility. The MaterialRequirement should be used to specify material requirements.

## Resource Identification

The schemas follow the ANSI/ISA-95 standard by defining resources by class ID or instance ID, or by defining them by class ID and a property value that is used to define a subset of the resource. For example, the figure below illustrates that a segment may require a certain number of milling machine, an equipment class. Other segments may require a subset of milling machine, such as “Fine” milling machines only. In the first case the class name, “Mill”, is sufficient to identify the resource required. In the second case the class name, “Mill”, and property name and value, “Spec” and “Fine”, define the required resource. Alternately a specific resource may be specified for a production schedule, such as requiring milling machine with ID=”Miller#1”.



# Element Definitions

| **Element/Type** | **Description** |
| --- | --- |
| ProductionSchedule  ***ProductionScheduleType*** | Contains a definition of a production schedule, including the location of the scheduled elements, the publication date of the schedule, the time range of the schedule, and the list of production requests that make up the schedule. |
| ProductionRequest  ***ProductionRequestType*** | Contains a definition of a production request element of a production schedule, including the associated product to be produced, the time range of the request, the priority of the request, the segment requirements of the request, and the definition of the expected segment response. |
| SegmentRequirement  ***SegmentRequirementType*** | Contains a definition of the schedule for a specific segment of production, including an identification of the associated product or process segment, the time range of the request, the expected duration of the request, production parameters for the segment, and the definition of the personnel, equipment, material produced, material consumed, and consumables to be used in production. |
| MaterialRequirement  ***MaterialRequirementType*** | Contains a definition of a material to be produced, consumed, or consumable material (non lot tracked material), including an identification of the use of the material, the quantity of the material or a definition of required subsets identified by resource properties.  A **MaterialRequirement** element may have a set of contained **AssemblyRequirement** elements to support hierarchical manufacturing bills. |
| MaterialRequirementProperty  ***MaterialRequirementPropertyType*** | Contains a definition of a subset of a material used in a segment requirement, including the value used to identify the subset and the quantity of the material used. |
| ConsumableExpectedRequirement  ***ConsumableExpectedRequirementType*** | Contains a definition of a consumable material used for a segment requirement, including an identification of the quantity of the resource consumed, or a definition of required subsets identified by resource properties.    *Note: This element is included for backward compatibility. The MaterialRequirement should be used to specify material requirements.* |
| ConsumableExpectedRequirementProperty  ***ConsumableExpectedRequirementPropertyType*** | Contains a definition of a subset of a consumable material used in a segment requirement, including the value used to identify the subset and the quantity of the consumable used.    *Note: This element is included for backward compatibility.* |
| EquipmentRequirement  ***EquipmentRequirementType*** | Contains a definition of an equipment requirement for a segment requirement, including an identification of the quantity of the resource used, or a definition of required subsets identified by resource properties. |
| EquipmentRequirementProperty  ***EquipmentRequirementPropertyType*** | Contains a definition of a subset of an equipment resource used in a segment requirement, including the value used to identify the subset and the quantity of the resource used. |
| MaterialConsumedRequirement  ***MaterialConsumedRequirementType*** | Contains a definition of a material to be consumed for a segment requirement, including an identification of the quantity of the resource consumed, or a definition of required subsets identified by resource properties.    *Note: This element is included for backward compatibility. The MaterialRequirement should be used to specify material requirements.* |
| MaterialConsumedRequirementProperty  ***MaterialConsumedRequirementPropertyType*** | Contains a definition of a subset of a material consumed in a segment requirement, including the value used to identify the subset and the quantity of the material consumed.    *Note: This element is included for backward compatibility.* |
| MaterialProducedRequirement  ***MaterialProducedRequirementType*** | Contains a definition of a material to be produced for a segment requirement, including an identification of the quantity of the resource produced, or a definition of required subsets identified by resource properties.    *Note: This element is included for backward compatibility. The MaterialRequirement should be used to specify material requirements.* |
| MaterialProducedRequirementProperty  ***MaterialProducedRequirementPropertyType*** | Contains a definition of a subset of a material produced in a segment requirement, including the value used to identify the subset and the quantity of the material produced.    *Note: This element is included for backward compatibility.* |
| PersonnelRequirement  ***PersonnelRequirementType*** | Contains a definition of a personnel requirement for a segment requirement, including an identification of the quantity of the resource used, or a definition of required subsets identified by resource properties. |
| PersonnelRequirementProperty  ***PersonnelRequirementPropertyType*** | Contains a definition of a subset of a personnel resource used in a segment requirement, including the value used to identify the subset and the quantity of the resource used. |
| PhysicalAssetRequirement  ***PhysicalAssetRequirementType*** | Contains a definition of a physical asset requirement for a segment requirement, including an identification of the quantity of the resource used, or a definition of required subsets identified by resource properties. |
| PhysicalAssetRequirementProperty  ***PhysicalAssetRequirementPropertyType*** | Contains a definition of a subset of a physical asset resource used in a segment requirement, including the value used to identify the subset and the quantity of the resource used. |
| ProductionParameter  ***ProductionParameterType*** | Contains a definition of a production parameter, which may correspond to a product segment parameter or a process segment parameter, including the value for the parameter. |

# Transaction Elements

The following elements are defined to support the ISA 95 Part 5 transactions, using the transaction data types defined in the B2MML-Common.xsd schema.

| **Production Schedule Elements** | **Description** |
| --- | --- |
| GetProductionSchedule | Get *ProductionSchedule* definition. |
| ShowProductionSchedule | Returned information from the *GetProductionSchedule* message. |
| ProcessProductionSchedule | Process *ProductionSchedule* definition. |
| AcknowledgeProductionSchedule | Returned status from the *ProcessProductionSchedule* message. |
| ChangeProductionSchedule | Change *ProductionSchedule* definition. |
| RespondProductionSchedule | Returned status from the *ChangeProductionSchedule* message. |
| CancelProductionSchedule | Cancel *ProductionSchedule* definition. |
| SyncProductionSchedule | Published *ProductionSchedule* definition. |

# Diagram Convention

The schema diagrams using the following convention to illustrate the structure of the schema elements, the type of the elements and attributes, and the rules for optional elements and repetition.



About MESA: MESA promotes the exchange of best practices, strategies and innovation in managing manufacturing operations and in achieving operations excellence. MESA’s industry events, symposiums, and publications help manufacturers achieve manufacturing leadership by deploying practical solutions that combine information, business, manufacturing and supply chain processes and technologies. Visit us online at <http://www.mesa.org>.

About the XML Committee: The XML Committe was formed within MESA to provide a forum for the development of the B2MML and BatchML specifications.